**ASSESSMENT ANALYSIS**

**Property Address:** **62 Wake Road S7 1HG**

|  |  |
| --- | --- |
| **Current EPC (Rating)** | D-55 (Exp July 2026) |
| **PRE-EPR Rating** | D-62 (000360) With SH |
| **POST-EPR Rating** | D-65 (000376) With SH |
| **Area** | 151m² |

**MEASURES TO INSTALL**

1. **IWI**

**NOTES FOR LOFT TEAM**

|  |  |
| --- | --- |
| **Pre-Condition** | 100mm |
| **Post-Condition** | 100 mm |
| **Extractor Fan Required** | NO, “see notes below” |
| **Trickle Vents Required** | Yes, (All WHITE colour) |

* **kitchen:** Please check if the kitchen extraction hub is in working condition. If not then install extractor fan in the kitchen.
* **Bath:** There is an extractor fan. please check it is working condition. if not then install it.
* **Trickle Vents:** Take proper photos of all trickle vents from inside and outside after install.
* **Elevation Photos:** Please take proper elevation photos after installation of trickle vents fan in day light. (Dark photos are not accepted)
* **Door Undercut: (**Please take a photo of the door undercut of the all bedrooms, both living rooms, bath, kitchen and RIR rooms**).** Bring two photos of each door undercut, one with closed door full view other with measuring tape under close door.
* **Measurement:** take photos of measurement from main entrance door and also from back extension (which has sloping roof).
* **Heating Controls:** Kindly take landscape photo of all radiators with TRV’S with visible both ends and also programmer and thermostat.

**NOTES FOR THE OFFICE**

* We will use existing EPC as On Gas proof.
* **Please get benefit letter**
* **please get land registry**
* **According to surveyor: customer did not allow me to drill in RIR for taking evidence. Customer and Surveyor say: RIR is insulated**